**MAINTENANCE:** Brush off any loose dirt and debris and rinse with water regularly. Clean with a solution of mild soap and warm water, using a sponge or soft brush. Rinse thoroughly and air dry. Keep any press studs free of salt and grit. Lubricate as needed with petroleum jelly for ease of use and longevity.

[www.covercraft.net.au](http://www.covercraft.net.au)

Ph 03 9729 3030