RSS COLD WATER PRESSURE WASHERS

Model 7423 – 7.4 GPM, 2300 PSI

Model 5530 – 5.5 GPM, 3000 PSI

Why Choose an RSS Cold Water Pressure Washer?

* Direct Drive Pump.
  + Having the pump coupled directly to the motor eliminates the need for belts or a belt tensioner, lowering your need for maintenance.
* 10HP Baldor® Motor.
  + USA Made
  + Totally Enclosed, Fan Cooled 220v, 1ph, motor ensures long life.
* Flat Free Tires
  + Never worry about flat tires again! Your washer will always roll to and from any location with ease.
* Powder Coated Finish
  + Professional, High Quality powder coated finish guarantees the best possible rust prevention.
* Industrial Annovi Reverberi (AR) Pump.
  + AR has been manufacturing high quality, Italian pumps for over 55 years. We only trust the best for your equipment!
* Industry Leading Service
  + Over 20 Years of experience to back up our equipment.

Standard Equipment:

* 36” Wand and Trigger Assembly
* 50’ x 3/8” 4000PSI Steel Braid Hose
* 15o Nozzle
* 25o Nozzle
* Quick Couplers on Pressure Washer, Hose, Wand, Trigger, and Nozzles

Optional Equipment:

* Low Pressure Soap injector
* Foamer
* 0o Rotating Nozzle