Image with Radiant Logo at top of leaflet:

Enjoy permanent mist free mirrors in your bathroom with Radiant Demister Pads

* Developed & manufactured in the UK
* Simple to install & use
* Economical to run
* 10 Year Warranty
* Maintenance Free
* IP44 rating

Mirror demisters are used by many if the world’s leading hotel groups & they are now available for your bathroom.

Available in 5 stock sizes

|  |  |  |
| --- | --- | --- |
| Product Code | Size | Wattage |
| RDM7020 | 574mm x 274mm | 28 watts |
| RDM7030 | 519mm x 527mm | 50 watts |
| RDM7035 | 790mm x 524mm | 77 watts |
| RDM7040 | 1004mm x 524mm | 100 watts |
| RDM7050 | 1506mm x 524mm | 150 watts |

Other custom sizes are available for multi units orders such as apartments & hotels, please contact us for details.

**How does the Radiant Demister work?**

When hot moist air is contact with a cold surface (like a mirror) condensation forms immediately on that cold surface. The demister works by simply raising the surface temperature of the mirror sufficiently so that condensation doesn’t form in the area that has been heated (typically increasing the surface temperature by 15 – 20 deg C). The mirror will feel warm to the touch, but the increased temperature will not cause any issues with the glass.

It usually only takes a couple of minutes for the demister to warm the mirror surface so by simply turning on the demister before taking a bath or shower, the mirror will remain mist free!

**Are they easy are they to install?**

Radiant Demisters are very simple to install. They have a self-adhesive coating which simply sticks to the back of the mirror. The electrician needs to make the connection to a switch & the mirror can then be hung or fixed to the wall in the normal way.

**How do I choose the best size for my mirror?**

Obviously you need to select a demister size that is smaller than the mirror & for most people demisting the main central area of the mirror is more than sufficient. So for example if your mirror is 1200mm wide x 800mm tall, then model RDM7040 at 1024mm x 524mm is ideal

For very large mirrors you can use 2 or more demister pads, but in most cases this is not necessary.

2 x drawings to go onto leaflet plus product photo: