The WorkStar® 2000 is a cordless, rechargeable high-performance LED work light with an articulating neck that lets you turn the light head and brightly illuminate your work space with over 300 lumens of brilliant white light! Attach it to any metal surface with 2 integrated magnets or hang it using the retractable hook! The WorkStar™ 2000 features a wide-angle, floodlight-style beam that illuminates a large area evenly, without hot spots or dark spots.

* Available in 3 body styles

The WorkStar® 2000 has 2 rare-earth magnets to attach to metal surfaces (upper magnet is hidden in picture by removable belt clip).

|  |  |
| --- | --- |
| **PARAMETER** | **PERFORMANCE** |
| **LED Brightness (Luminous Flux)** | High > 300 emitter lumens, Low > 75 emitter lumens |
| **LED, Color, Power** | Cree XP-G, Cool White, 5 W |
| **Heat sink** | LED and lens are mounted in a sealed aluminum heat sink assembly, which protects the LED from dirt and fluids |
| **ON/OFF HI/LO Power/Brightness Switch** | Recessed ON/OFF push button switch also controls 2 brightness levels |
| **Favorite Brightness Level Memory** | Turns ON and OFF to your favorite brightness level, yet easy to change to the other level |
| **Batteries Included** | 6 AA rechargeable NiMH battery pack |
| **Run time per charge** | High > 2 hours, Low > 8 hours |
| **Recharge Time** | About 6 hours |
| **Regulator Circuit** | High efficiency constant current circuit to maximize brightness and runtime |
| **Charge/discharge Indicator** | A bicolor LED charge/discharge level indicator flashes green and red to help you estimate the remaining runtime and recharge time |
| **Lens** | Unique "fresnel-like" lens provides a smooth beam of light with no hot spots |
| **Glass Lens** | Tempered glass with a shock absorbing rubber gasket |
| **Material** | High impact PC, except neck and hook, which are glass reinforced ABS |
| **Flared Base** | Stable when standing upright thanks to the wide flared base |
| **Hand Grip** | Comfortable ergonomic hand grip |
| **Head Rotation** | Head rotates 360 degrees with smooth stop-notch action |
| **Head Tilt** | Tilts 180 degrees and has a tension adjustment screw that prevents head from flopping |
| **Retractable Hook length** | 3 inches (7.5 cm) when extended; retracts into body |
| **Hook diameter** | 1 inch (2.5 cm) |
| **Magnets** | 2 powerful, co-planar, nickel-plated, neodymium rare-earth magnets |
| **Belt Clip** | Better than holster, this belt clip lets you use the light while clipped to your belt. It quickly clips onto the light and slips off just as easily, but sticks securely while in use. |
| **Tripod** | Standard camera tripod socket in base |
| **Overall length** | 10 1/4 inches (26 cm) |
| **Body Dimensions** | 6 3/4 x 2 x 2 inches (17 x 5 x 5 cm), anti-roll surfaces |
| **Head Dimensions** | 3 x 1.5 x 1.5 inches (7.5 x 3.8 x 3.8 cm) |
| **AC Power Supply** | 100-220 VAC 50/60 Hz UL-Approved North American power supply with standard "Type A", two prong plug |
| **Car Charger** | 12 VDC car adapter |
| **What's Included** | WorkStar 2000 with rechargeable NiMH batteries, 100-220 VAC power supply, 12 VDC car adapter, belt clip |
| **Weight** | 1 Lb. (0.5 kg) |

Gearhead’s Floodlight

Order No. MXN02040

Imitation carbon fiber coating



Hunter’s Floodlight

Order No. MXN02030

Realtree™ Camo coating


Insert REALTREE AP logo



Technician’s Floodlight

Order No. MXN02000











**WorkStar®** Technician’s Floodlight