  
  
**5 - IN - 1 CURLING WAND**  
  
FIVE INTERCHANGEABLE CLIP-FREE TOURMALINE BARRELS INFUSED WITH TITATNIUM  
  
5 SIZES IN THE SET:  
32MM 25MM 13/25MM 19MM PEARL WAND  
  
TEMPERATURE CONTROL:  
AUTOMATIC SHUT OFF TIMER  
READY IN SECONDS, NO MORE WAITING!

250-450°F / 100-230°C  
  
VOLTAGE:  
110-240V

THIS SLEEK DESIGN IS DURABLE AND CREATES THE SMOOTHEST, SOFTEST CURLS WITH NO BREAKAGE OR CREASES!  
  
THE TOURMALINE INFUSED BARRELS WITH INFUSED TITATNIUM PRODUCES HEAT FOR GENTLER, PROTECTIVE STYLING!

INFRARED AND NEGATIVE ION TECHNOLOGY LEAVES NO FRIZZ!  
  
ONE YEAR WARRANTY INCLUDED  
