Heavy Duty Lab Benches

Standard Lengths (inches): 36, 60, 72 and 84. Standard sizes ship faster. Open design allows room for chiller underneath. Custom depths, custom heights available. Tolerances on custom sizes is ¼”. Shorter heights may be better for taller instruments, or custom length to fit in the exact area in your laboratory.

**Construction:** benches are steel frame (3 inch legs, 1.5 inch cross beams; 0.188 inch heavy duty steel); 6 inch heavy duty casters (with locks on all four wheels). 1/8” metal x 1.5” bars under bench top for mounting of optional accessories. 1000 kg weight rating. Made in Canada.

**Durcon tops:** (see <http://www.durcon.com/sites/durcon/files/docs/resources/SPC%20Specification.pdf>) for chemical resistance and other specifications. 1” thick material.

**Options:**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Default** | **Other Options** |
| Colour | White | Black |
| Corners | Rounded Corners | Sharp Corners |
| Feet | 6” Heavy Duty Casters | Adjustable Feet |
| Keyboard | Left Side | Center or Right |
| Computer Cradle | Left side | Right Side |
| Pump Cabinet | Right side | Left side |
| Length | 72 inches | 36, 60, 84 |
| Depth | 30 inches | 36 |
| Height | 35 inches | 30 |
| Clearance under table | 32 inches | 27 |

 

Benches are powder coated (white or black). Benches can be left open underneath for storage or chillers, or an optional pump cabinet (insulated with integrated fan) added.

Optional monitor stands, heavy duty keyboard trays, or under the counter PC cradles can be added.

**Ordering Information**

|  |  |  |
| --- | --- | --- |
| **Model** | **Details** | **Production Time** |
| LB-36 | 36” long, no cabinet | 3 weeks |
| LB-60 | 60” long, no cabinet | 3 weeks |
| LB-72 | 72” long, no cabinet | 3 weeks |
| LB-72C | 72” long, **with** pump cabinet | 4 weeks |
| LB-84 | 84” long, no pump cabinet | 1 week, normally stocked |
| LB-84C | 84” long, **with** pump cabinet | 4 weeks |



84” bench with Durcon top. Top is larger than frame by two inches on all sides. Clearance under the frame is 32” on a 35” tall bench. Benches ship on a wooden pallet completely assembled, but can be disassembled for tight doorways.

**Contact Details:**

Fonebone Services Inc. (780) 267-3555 [www.fonebone.ca/benches](http://www.fonebone.ca/benches)