Ladies and Gentlemen,

Thank you very much. You have done a wonderful job for our company. Here are a few last modifications we would like to see after our team review. We are very happy with your design and look forward to the completed version. Thank you again…Jim Turner

Wording change for *Introduction…*

Nichigo G-Tape is an innovative family of acrylic tapes manufactured by Nippon Gohsei, USA. Nichigo G-Tapes provide superior performance in construction and industrial applications while being versatile enough for household tasks. All Nichigo G-Tapes series share the unique feature of being hand tear able. Nichigo G-Tapes can be separated into two major categories: Hard surface protection tapes featuring residue free removal, and Permanent adhesion high performance tapes and flashing. Welcome to Nichigo G-Tape.

Brief descriptions under tape photos (layout and black box/white print headers keep as is)

INDUSTRIAL / CONSUMER SERIES PRODUCTS

1009GR (Green)

Premium hard surface protection tape…No residue removal from most surfaces…Hand tear able…Waterproof…Chemical resistant…Solvent acrylic adhesive…Available in Clear.

2010BL (Blue)

Low residue, excellent adhesion multi-purpose acrylic adhesive tape...~~Good~~ Strong initial tack…Hand tear able Waterproof…Chemical resistant…Available in Black, Yellow, Red, Beige, and Gold.

2010AL (Silver)

HVAC and insulation seaming tape… Hand tear able…No cutting tools needed…Safer tape edge than aluminum foil tape…ASTM E84 (UL723) Class 1 Flame spread ~~40~~ -4°- 190° F application temperature.

9014CL (Clear)

Double sided clear tape…Ideal for seaming and splicing…Straight clean tearing…Perfect for arts and crafts ~~as well as~~ and DIY projects. Permanent bond after initial period of being repositionable.

This description below was missed in the versions you sent. It was a repeat of the 9014 CL

5009MTBK (Matt Black)

Gaffer’s Tape…Unique acrylic G-Tape formula means no residue when removed from most surfaces, including cables where residue can cause ruin…Matt black in color for low reflection… Hand tear able …Very strong and stable.

1008SW (Snow White)

Marine Grade Tape…Use where high UV resistance is a priority…Clean, residue free removal after 5-7 months of sunlight exposure…Wide application temperature -~~40~~ -4°- 190° …High chemical and solvent resistance.

CONSTRUCTION SERIES PRODUCTS

2020SB (Sky Blue)

Superior House Wrap and Insulation board seam tape…Outstanding tack and long term adhesion…Hand tear able…Many contractor friendly features…Priced competitively to standard “plastic” tapes…Wide application temperatures -4°--190° F …Available in 2”and 3” width rolls.

3030BK (Black)

Commercial grade Building Wrap and Insulation seaming tape…Highest overall performance values…Excellent long term (25+ years) performance…. Adheres to difficult surfaces where standard tapes fail…Clean straight tear by hand…No waste as face/face contact can be easily separated with no performance loss… Wide application temperatures -4°-- 190° F…also available in white.

9030BK

Double sided version of 3030BK…Seals overlapped seams…Use wherever permanent double sided adhesion is needed…Hand tears clean and straight…Used in hardwood flooring installation and other construction trades. Available in 1” and 2” roll widths.

3040BK (Black)

Exceptional acrylic adhesive performance with unmatched contractor friendly features…AAMA 711-13 Level 3 Class A…Highest Standard Available…Meets standard without the need of primer…Lighter weight- 50-70% lighter than rubber asphalt or butyl flashing r~~esulting in less jobsite fatigue~~…Hand tears clean and straight… Wide application temperatures -4°-- 190° F … No waste as face/face contact can be easily separated with no performance loss… Repositionable… Becomes permanent after 24hrs… 50 year tested adhesion values still exceed code requirements…Uses include flashing for windows, doors and other wall openings… 3040BK is a favorite of professional deck builders as it is chemical and solvent resistant…Available in 2”, 4”, 6”, 9”, 12” and 51” roll widths…Also available in White.

Page 4

**Representative Values Table**

\*\*\*IMPORTANT\*\*\*Add a line under the table. Does not have to be large print but must be readable that says **“Typical values, not for specification or guarantee purposes. Contact manufacturer for design specifications”**

**Also in table in the Roll Size(s) row – stack the sizes wherever you can to create a more symmetrical box width. Some were stacked and some were on a single line causing the column width to change. Individual Box borders are also faintly showing in some of the boxes.**

**Last row needs the format for the months changed to text as the boxes appear to be dates (I assume you already caught this but just a reminder…jt)**

**Spelling in Text under the table and left of the diagram**

**Change all “&”s to “and”**

**Place a period after …adhesive bonding.**

**Change NEGTIVE to NEGATIVE**

**Change ATTRACT to ATTRACTED**

**Replace comma after MAGNET with period and space.**

**Replace last sentence with the following**

**“THIS COMBINES WITH HEAT TREATED POLYETHYLENE CORE TO INSURE A TIGHT WATERPROOF SEAL”**

**WE prefer the white version of the Vandermeer Logo**

**Expand the “label” area in the lower right hand corner to leave smaller red border. 1/16” border of red on rt side and bottom should be fine. Possible use a shaded area without a border as an option. Use your own judgement.**