Gyprocker/PLASTERERS apply and fix plasterboard partitions, suspended ceilings, fire rating systems, acoustic tiles, and composite wall linings to buildings, and apply decorative and protective coverings of plaster, cement and similar materials to the interiors and exteriors of structures.

determining plasterboard layout, and installing insulation and vapour barriers

measuring, marking and cutting plasterboard, lifting and positioning panels, and securing them to walls, ceilings and battens

preparing corner beads and securing them in position

fixing pre-cast cornices, panel mouldings, ceiling centres and other plaster fittings

covering joins and nail holes with wet plaster and sealing compounds, and smoothing them using wet brushes and sand paper

mixing and applying coats of plaster, cement and render to structures using trowels, and levelling and smoothing coats to uniform thickness

plumbing and straightening corners, angles and wall and ceiling surfaces

creating decorative textures in finishing coats

applying and finishing acoustic, insulating and fireproofing materials bonded with plaster, plastic cement and similar materials