Tower Charger Station Host

Model: GC-32-RF

Product placement: Hotel room, Conference, Office, Café, Lounge, Bar, Club, Restaurant

Brand name: Generation Charge

Host input: DC 5V/1A

Host frequency: 433mHZ; Max power: 20dBm

Host capacity: 1000mAh/5Wh

Certificate: CE/RoHS/CE/FCC/UL

Delivery time: 1-3 weeks

Advantages:

Anti-lost: the host can be set at a specific distance range to control the chargers.

Wait in line: A charger could be recorded in the host, and then queue up.

Call for service: press on the charger button and call the host for service