**TECHNICAL PRODUCT INFORMATION**

**V40 Pro (spray)**

**Application:**

V40 Pro is a high grade multifunctional product for lubrication and protection product.

V40 Pro is composed out of high grade synthetic oils, E.P. additives and penetrants. Also the product contains rust-preventing and waterproof substances. Practical experience proofed that V40 Pro cleans, lubricates and protects equipment, hinges, cables, conveyer belts, chains and other moving parts in machines and device excellently. V40 Pro cleans fats, resins and rust on the surface of materials.

V40 Pro create a good and durable lubrication. Even under circumstances with extreme pressure.

V40 Pro protects against moisture and rust.

**Instructions for use:**

* Short shake before use
* Spray a thin layer of V40 Pro on the surface. The product will come out as a white, fast disappearing foam.
* Let V40 Pro do its work for a few minutes.
* Own evaluation for necessity and result.

**Special advantages:**

* V40 Pro drives off the eventually present moisture.
* V40 Pro can handle temperatures until 370˚C.
* V40 Pro reaches even the smallest corners. This is because of the pressure of the spray, foaming and presence of high grade penetrants.
* V40 Pro forms an extremely thin and smooth layer of grease (Fw value: 0,1).
* V40 Pro helps prevent “pitting wear”.
* With use in propulsions, the starting couple will be lowered.

**Specifications:**

Colour: Yellow

Density: 1,07 g/ml

Temperature range: -40 until 370˚C