Brochure edits 22/6/20

Back page:



* The size of the capping are all different. Heritage and Bevelled capping are larger than Bullnose and Colonial even though they are made from the same thickness of material (32mm). Please make bullnose and colonial the same size as heritage and bevelled.
* The angle of the Dental is not at the same angle as the other designs.



Change the purple flute to a shade of grey (same colours as the doors).






Crop this image

The new 3D Wall panels photo on the right needs to show the cabinets not the sink. Please show this part of the doors. Make sure to line it up with the logo and the photo on the left.

Page 3:



The doors should be in order of their 3 letters as the letters indicate the design. Please place them in this order:

6009 KSQ, 6008 PSQ, 6009 PSQ, 6010 PSQ, 6011 PSQ, 6009 XSQ,

6001DSQ, 6001 ISQ, 6002 ISQ, 6003 ISQ, 6003 JSQ, 6001 MSQ, 6001 TSQ,

Page 5:

Page 04 Range 5000

Please place doors in this order:

5001 BSQ, 5006 BSQ, 5001 DSQ, 5006 DSQ, 5106 DSQ

5001 MSQ, 5001 SQ0, 5101 SQ0, Drawer bank, Angled door

Page 05

4001 GSQ appears shorter than the other doors.

4001 HSQ and 4001 MSQ and 4001 FSQ - the top or side of the door is visible in the close up - zoom out a little more.

Please place doors in this order:

4001 ASQ, 4001 BSQ, 4001 CSQ, 4001 DSQ, 4002 DSQ, 4001 ESQ


4001 FSQ, 4001 GSQ, 4001 HSQ, 4001 LSQ, 4001 MSQ, Drawer bank, Angled door



GSQ is shorter than others

Top of door is visible in close ups HSQ and MSQ

Page 7:




1002 E

* Doors in range 1000 and 2000 are smaller than handles. Make the doors larger by reducing the white space between them.
* Change 1001B at the end of the range to 1002E



Design 1001 B - the side of the door is visible in the close up - zoom out a little more.

Order: 1001 2 Pin, 1001A, 1002A, 1001B, 1002E, 1001J, 2002F



Make spaces between frames equal

Please space the frames evenly