

**ACHS Clinical Indicator User Manual 2012 Intensive Care version 4**

7.2.16 Library facilities – an appropriate range of bench manuals , textbooks , journals and access to electronic medical information should be available 24 hours a day within the unit complex.

8.3 Protocols and in-service training for medical and nursing staff need to be available for the use of all equipment , including steps to be taken in event of a malfunction

**AORN : RECOMMENDED PRACTICES**

RP for Electrosurgery 2.8 March 2012

Read and attach the manufacturer’s manual to the unit or cart on which the ESU sits (pg 375)

During the use of AEC ( Argon enhanced coagulation technology) , all manufacturers written instructions should be followed in addition to all safety measures for monopolar surgery .

**Australian and New Zealand College of Anaesthetists (ANZCA)**

PS31BP 2012 Guidelines on Checking Anaesthesia Delivery Systems

It is the responsibility of each facility to ensure that specific checklists are available in accordance with manufacturers’ guidelines, for each item of equipment relevant to anaesthesia delivery systems.

**AS/NZS 4173:2004 Guide to the safe use of lasers in health care**

SECTION 9 SAFE PRACTICES

9.2 (j) The laser safety rules and equipment instructions are required to be made available at the site of use .

**Australian / New Zealand Resuscitation Council :Guideline 11.4 Dec 2010**

Electrical Therapy for adult advanced life support

Care should be taken to ensure that the pads or electrodes are applied in accordance with the manufacturer’s instructions …..

|  |
| --- |
| **STATE CORONER VICTORIA** |

Coroner’s “Investigation Standard”: Fall-related deaths in hospital

Relevant Equipment or work practice ( pages 2 )

b) If a particular product was involved, were the manufacturer's instructions available and followed? (If not why not?).