Instructions for installing

**STRIKE PLATE LOCKS**

TOOLS NEEDED:

One Phillips screwdriver

INSTALLATION:

1. Remove two screws from existing strike plate

2. Remove existing strike plate and replace with "**STRIKE PLATE LOCK"**

3. Secure "**STRIKE PLATE LOCK**" with our 2 inch security screws