**Versa-King framed modular construction offers distinct advantages for build out of cultivation facilities.**

Assembly time is reduced by as much as 75% over conventional construction.

Solid core laminated panel compositions provide excellent insulation values, are impact resistant, easy to clean, and will not support mold growth or insect infestation.

Our framed modular construction utilizes load bearing, corrosion proof connecting posts that seal tight onto panel surfaces to create a superior grow environment.

All rooms are designed as stand-alone structures. Ceiling systems don’t require the support from the existing structure and can be load bearing to support all mechanical equipment.

Virtually eliminate dust and debris for a cleaner construction site, reducing the cleanup time necessary prior to commencement.

A wide variety of wall panel compositions and finish options, including vinyl covered drywall for build out front offices, breakrooms, locker rooms and more.

**I suggest moving these images to the bottom of the ad and use the following captions:**

Other prefabricated construction solutions for grow facilities:

Structural steel observation towers – provide unobstructed view of outdoor grow operations

Factory assembled security buildings – secure entry and perimeter security points