**SUNSTATE COMMERCIAL CRUSHING AND SCREENING**

**MOBILE CRUSHING SERVICES**

**We Crush**

* Concrete
* Brick
* Blocks
* Asphalt
* Natural stone (sandstone, limestone and more)

**Technical Capability**

* **Production:** 5–50 tonnes per hour (dependent on feed & output settings)
* Maximum feed size of a single lump is500 mm × 280 mm but for best performance **300mm material is preferred**.

**MOBILE SCREENING SERVICES**

**We Screen**

* **Concrete**
* **Brick**
* **Stone**
* **Soil**
* **Sand**
* **Gravel**
* **Other construction & demolition materials**

**Accurate separation into fines, medium, and oversized**

**042 313 6655**  
 **info@sunstatecommercial.com.au**  
 [**www.sunstatecommercial.com.au**](http://www.sunstatecommercial.com.au)

**Color palette (matched to your logo)**

Dark Green: #0B5D2A

Light Green: #8BC34A