DIRECTIONS FOR USE


The surface must be thoroughly cleaned and free from grease, oil, dirt and moisture.

Protect surrounding areas from overspray. 

For best result ensure can is at room temperature. 

Shake can well before use.  

Hold can upright approximately 15-20cm from the surface. 

Direct nozzle away from people, point towards application surface.

Press nozzle firmly, apply light even coat to the surface. 

For best results apply light even coats and allow to dry between coats. 

Allow coats to build up to achieve desired result.

Avoid over application to prevent running and uneven drying. 

Rubber Wrap can be peeled off when dried, for best results apply sufficient Rubber Wrap to allow for easy removal and protection. 

