Page One

* Maxfield Program Benefits
* Picture of nurse wagon
* Web Site – www.maxfield.ca

MaXfield Field Nurse Tank

Inspection Program

MaXfield field nurse tank inspection program is an all-inclusive inspection service to improve equipment safety and industry compliance. MaXfield’s team of engineers, quality assurance inspectors and maintenance technicians have developed a leading preventative maintenance program that delivers;

* Industry Code of Practice compliance assurance
* Transport Canada CSA B620 compliance assurance
* Annual lump sum fee on per tank bases inclusive with all travel, subsistence, and labour cost.
* Access to MaXfield equipment online automated tracking system (OATS). This online secure data bank user interface allows equipment records to be sorted by location, capacity, Canadian or National Board registration number, or inspection due date. All inspection and maintenance records can also be down loaded and printed from program
* Long term scheduling to ensure all equipment is field ready prior to application season
* Program participant receive preferred service status with after hour call service
* Program participant loyalty programs
* Access to engineering for equipment up-grades, repairs, and modifications

Page 2

**Field Nurse Wagon Inspection Scope included In Annual Inspection Fee**

Annual Hose Test

* Hydro pressure of applicator transfer hose to 1.2 design pressure (420 PSI).
* Function test of passive shut down system when applicable. (ESV devise on currently installed on twin and Spec TC 51 wagons).
* Paint touch up of hose end valve to Code of Practice standards
* Supply and installation metal hose test tag with serial tracking number, test pressure, test date, and hose tester ID.
* Completion of hose test inspecting document.
* Posting of hose test inspection document on asset home page on MaXfield Online Automated Tracking System (OATS).

Two/Three Year Visual Inspection

* External visual inspection of vessel shell, attachments, impact guards, gauging devises, nozzle valves, pressure relief devises, labeling, and running gear.
* Paint touch up of valves and connection points as per Code of Practice standards.
* Supply and installation of inspection markings on vessel
* Completion of visual inspection document
* Posting of hose test inspection document on asset home page on MaXfield Online Automated Tracking System (OATS).
* Up-dating of asset photos on asset home page on MaXfield Online Automated Tracking System (OATS)

Five Year Pressure Test

* Hydro pressure test of vessel to 1.5 times design pressure.
* Function test of nozzle tank connection excess flow valves.
* Removal of hydro test water. Hydro test water drained to ground in owner facility.
* Installation of all new pressure relief valves.
* Supply and installation of metal relief valve ID tag with serial tracking number, installation date, and work order number
* Completion of pressure test inspection document
* Posting of inspection document on asset home page on MaXfield Online Automated Tracking System (OATS).

**All Inclusive Annual Inspection Fee $ 230.00 per tank\***

MaXfield Locations

Manitoba

386 Park Avenue

Brandon, MB R7A 7A8

Phone 204-571-6812

Saskatchewan

801 – 50th Street East

Saskatoon, SK S7K 3Y5

Phone 306-242-8900

Alberta

1026 Western Drive

Crossfield, AB T0M 0S0

Phone 403-946-5678

\*Does not include Nurse Wagon maintenance parts or installation