(Note to designers: Some or all of the content below may be used.  The below content is also in no particular order or layout)

HLG 550 

High Intensity LED Grow Lights


1000 watt HID Replacements


Double-Ended Replacements


Powered by Quantum Board Light Engines

 ~ Made in the USA ~

Goodbye HID's.


I'm sorry it's been that way for decades.


I'm no longer in need.

True 1000 watt HID SE and DE replacements.  
High Efficiency Modular Light Engines powerful enough for Big Ag & Hobby Horticulture.  

The HLG 550 indoor horticulture LED grow light is designed to replace a single ended 1000W HID.  Each lamp uses 4 custom designed high efficiency white light Quantum Boards. With a total of 1152 Top Bin Samsung LM561C S6 LED's, this fixture produces 1265 PPF with just 510 Watts.

Standard Issue Comes Clear Anodized Aluminum

TOP FEATURES

High efficiency white light Quantum Boards
White Light Full Spectrum for better results than HPS
Reliable passive cooled design
Better canopy light penetration with diffused light
Ideal for veg and bloom
Dimmable Power Supply included


Lead time: 1 week 

SPECIFICATIONS

Power	250-515 Watts
Voltage Range	90-277 VAC
LED	1152 pcs Samsung 561C
Flowering Footprint	            4.5'X4.5' or 4'X5'
Veg Footprint	6'X6'
System Efficiency	161 Lm/W
System PPF Efficacy	2.4 µmol/joule
Total output	1265 PPF
Dimensions	26"X20"x3"
Recommended Mounting Height	18-28 inches
3000k Spectrum Standard
 
Please contact for other spectrum options, 240V or UK, EU Power cords and wholesale or volume pricing.

Horticulture Lighting Group, LLC

865.770.1231

752 North State St
PMB 208
Westerville, OH USA 43082