Simradios

Simulated Radios

Affordable voice networking solutions for Windows-based computers

We Offer:

* Off-the-shelf, Plug-and-Play components
* Custom Communication Systems

Supports: Windows Vista, 7, 8, and 10

Compatible with most headsets, handsets, helmets, microphones and Push To Talk (PTT) devices

Highly scalable: Up to 16 users per PC.

Several models available, to support a variety of standard plug types such as:

* WE-425, PJ7 or “310 connector”
* U-283/U, Combat Vehicle Crewman (CVC)
* XLR4F, XLR3M, XLR5M, VXLR5F(Airbus), and XLR6M
* mil spec PJ-068 (M642/5-1) .206” microphone
* mil spec PJ-055B (M642/4-1) .25” headphone
* mil spec U-92/U(TJ-120), U-174/U
* Flexibility: Easily integrates with most third-party communications systems, radio applications, and VoIP programs
* Variety of defense industry standard IEEE 1278.1A-1998 Distributed Interactive Simulation (DIS) network radio communications applications
* Ruggedized for communications systems in the field or simulated training environments
* Easy four-way PTT communications. Ideal for dispatcher, emergency operations, command centers and simulation Instructor Operator Station (IOS)
* Supports USB 1.1 and 2.0
* Zero-latency sidetone
* Detects up to four PTT buttons per user
* No batteries or external power required

Some of our customers include: Adacel Systems, Area 51 ESG Inc., Australia's Department of Defence: Defence Science and Technology Organisation, Automated Business Power, CGI Federal, Datron World Communications, En-Net Services, Flight Training Europe, iGov, Northrop Grumman Corporation, SAIC, U.S. Air Force, U.S. Army, U.S. Joint Communications Support Element, U.S. Marine Corps, U.S. Special Operations Command South

CAGE Code: 6VL79

www.simradios.com