****

**ProSeries**

【Product Description】

A premium, eco-friendly, water-based paint for interior ceiling and wall application.

PACT’s ProSeries line delivers the high quality results that professionals love whilst maintaining the lowest levels of odour emissions and VOC content.

【Features】

* Low VOC content
* Low Odor levels
* Super Adhesiveness
* Scrub Resistant
* Anti-Moulding effect
* Water-Washable
* Self-Priming
* Fast Dry Time
* Flexible Application
* Long-Lasting Colour

**Low Sheen White 18L**

【Application Tools】

Brush, roller, spray.

【Application condition】

Surface must be clean, dry and free from dust, oils and grease.

Apply two coats ensuring that the first coat is completely dry before applying the second.

【Application Instructions】

1. Add 20% water in the paint, stir evenly in a circular lifting motion for before use

2. Apply two coats on/in application tool

3. Use primer[1] on dry wall and leave to dry

4. Brush the wall with the paint as a finish (recommended two coats)

5. Average dry time is 24 hours. If the weather is cold and wet, the dry time will be longer. Fully cured time is 7 days in summer, 15 days in winter.

**Remarks**

[1] If you don’t have a primer product, you can use this paint as a primer. In other words, the paint can be used as both a primer and finisher.

【During Painting】

Ensure adequate ventilation. Keep floors and furniture covered

【After Painting】

Avoid exposure to steam for 48 hours

Surface may be washed after 7 days

【Coverage】

Coverage Rate: Approx. 10m2/KG for 1 coat on wall

Approx. 5 m2/KG for 2 coat on wall

【Disposal】

Do not pour leftover paint in drains or sewers. Keep unwanted paint in sealed containers to be disposed via chemical waste collections. Unwanted paint can be brushed onto newspaper allowing time to dry then disposed via domestic waste collections.

**DO NOT REUSE CONTAINER UNLESS THOROUGHLY DECONTAMINATED**

【Safety and First Aid】

**For spills and disposals:**

Slippery when spilt, clean up immediately. Refer to Local Authority for disposal advice. Do not empty into drains and waterways.

**First aid:**

If poisoning occurs, contact a Doctor or Poisons Information Centre AUST 131 126

**Eye contact:**

If contact is made with eyes, hold eyes open, flush with running water for at least 15 minutes.

**Skin contact:**

If contact is made with skin, remove any contaminated clothing and wash skin thoroughly.

**If swallowed:**

Rinse mouth with water, DO NOT induce vomiting

**Clean up:**

Wash up with water. Do not dispose of paint or wash water in drains or sewers

**ALWAYS KEEP OUT OF REACH OF CHILDREN**