

**“The General” By Patriot Hitches, LLC - Specifications**

* **Ball And Accessory Mounts**
* Meets Or Exceeds J684 SAE Testing Standards
* Ideal For Marine, Agricultural, Recreational And Of Course - Military Use
* Adjustable - Matching The Height Of Your Application
* Lifetime Warranty
* Sturdy Steel Construction
* Black Powder Coat Finish Resists Rust And Corrosion
* Simultaneous - Use Accessory Attachment Option  
  (See “The Specialist” Accessory)
* Max GTW = NEVER Exceed Your Vehicle Limits

By The Numbers….

* Maximum Rise: 11” / Minimum Rise 3”
* Maximum Drop: 11” / Minimum Drop 2”
* Adjusts By 1-1/2" Increments
* Full Adjustment Capability 22”
* Shank Length 6” - Hole Position 2 1/2”
* Hitch Coupler Has 2-Hole Positions For Optimum Use
* 2 Anti-Tilt And Sway Locks
* Fits 2” Inch Hitch Coupler
* Fits 2 ½” Inch Hitch Coupler (With Reducer Insert)
* Class III
* 8000 LBS Max GTW
* Gross Towing Weight: 6,000 LBS At Max Drop.
* Gross Towing Weight: 8,000 LBS At Min Drop.
* Tongue Weight: 600 LBS At Max Drop
* Tongue Weight: 800 LBS At Min Drop
* Hitch Weight 15 LBS.
* Hitch Max Width 3”
* Overall Length: 11 ¼”"-
* Overall Height: 13 ¾”
* Shank Size: 2"
* 4 Pins (5/8) And 4 Clips Included