**Front of box:**

CRYSTALUMIA ™ Logo

Chandelier Crystal Bulbs

LED Technology

<Product Photo>

2700 K = Warm White

Non-dimmable

3 PACK

Model: DQ51E12ND27K120V

4.3w

300 lm ~ 30w equivalent (7 times more efficient than incandescent lamps)\*

15,000 Hours average lifetime\*\*

90% Energy Saving\*\*\*

Lasts 13 years\*\*\*\*

PF > 0.9

CRI > 80

No Radiation

Flicker-free

100% Instant Glow Start Up

CE

IP20

Beam Angle > 330°

Never fog

Ø40 x H95 MM

AC 110-120V

Base type: E12 Candelabra

\* Lumens are representative of an average of measured value.

\*\* LED lifetime in 25°C operating environment. The expected average lifetime in residential use is 15,000 hours.

\*\*\* Energy Saving is a guide only based on an incandescent lamp with an equal Lumens output.

\*\*\*\* Based on 3hrs/day (13.70 years)

**Back of box:**

<Colour Temperature Chart> photo

<Lighting Facts> photo

Barcode: 9369998025794

Product ID: CLED-DQ51-E12-ND-27K-120V-3P

Caution: This device is not intended for use with emergency exits. Risk of Shock - Do not use where directly exposed to water. Turn off power before inspection, installation or removal. Not for use in Totally Enclosed Fixtures. Use in open luminaire only. Use only on 120 Volt, 60 Hz circuits. Not suitable for use with dimmer switches.

2 Year Warranty

CRYSTALUMIA ™ brand, logo and this packaging is subject to copyright and must not be reproduced, copied or otherwise used in any way or for any purpose without consent in writing of the owner.

Please Recycle (Recycle Sign)

Made in China

**Right Side of Box:**

<Energy Consumption Rating> photo (Needs customisation)

Distributed by:

Distribution International

17 Pannell Road

Bateman WA 6150

Australia

For assistance, please visit:

www.crystalumia.com

**Top Side of Box:**

CRYSTALUMIA ™ Logo

Chandelier Crystal Bulbs

Model: DQ51E12ND27K120V