Introducing the Z Poolform System.

For creating a seamless and architectural concrete pool coping surround.

Available in Australia and New Zealand from Concrete Countertops Australia.

Don't waste your time with fiddly, flimsy, or time consuming pooledge forming systems that end

up in landfill. The Z Poolforms are made from strong PVC and can easily and quickly produce architectural designed looks that suit all types of pools.

* Quick and easy to form saving labour time
* An average size pool can be formed up in 2 - 3 hours
* Tough but smooth PVC means great results and less time honing, cutting back, or patching uneven concrete
* Forms come in both straight and bendable so will suit any shaped pool.
* Will suit all pool types - Fibreglass, concrete, or vinyl lined
* Suitable for new pools or poolside refurbishments
* Best of all, the forms are reusable which makes subsequent pools much cheaper to pour

Since we introduced this product into the market four years ago, there has been an increase in the demand from clients looking for a seamless, architectural concrete pool surround. While there are several different methods for achieving this look, the Z Poolform System is the easiest to use with the best results.

Forms

Z Poolforms w/ Square Poolform Backing - Straight and Bendable

Z Poolforms - For use with rubber form liners

Receiver Track - Straight and Bendable

Pool Liners - Coping face edges include Bermuda, Bullnose, Bullnose Slate, Chiseled Slate, and Chiseled Stone

Accessories

Finish off an amazing look with

Receiver Trim

A Concrete Skimmer or Drain Lid from HIDE

